**General**

|  |  |  |  |
| --- | --- | --- | --- |
| **Frequency coverage (Unit: MHz)** | **Receiver** | 0.030–199.999\* 400.000–470.000\* | |
| **Transmitter** | 1.810–1.999 3.500–3.800 7.000–7.200 10.100–10.150 14.000–14.350 18.068–18.168 21.000–21.450 24.890–24.990 28.000–29.700 50.000–52.000 144.000–146.000 430.000–440.000 | |
| **Mode** | | USB, LSB, CW, RTTY, AM, DV, FM, WFM (Rx only) | |
| **No. of memory channels** | | Memory channels: 500 channels (100 groups)  Scan edges: 25 channels  Call channels: 4 channels (2 channels x 2 bands) | |
| **Antenna connector** | | BNC connector (50Ω) (One connector for all bands) | |
| **Power supply requirement** | | 13.8 V DC ±15% (with external power supply)  7.4 V DC (with BP-272) | |
| **Operating temp. range** | | –10°C to +60°C; +14°F to +140°F | |
| **Frequency stability** | | Less than ± 0.5 ppm  (–10°C to +60°C; 14°F to 140°F) | |
| **Frequency resolution** | | 1 Hz | |
| **Current drain** |  | **13.8 V DC** | **7.4 V DC** |
| **TX (Max. power)** | Less than 3 A (10 W) | Less than 2.5 A (5 W) |
| **RX (Max. audio)** | 0.5 A (typical) | 0.8 A (typical) |
| **RX (Standby)** | 0.3 A (typical) | 0.5 A (typical) |
| **Dimensions** | | 200×83.5×82 mm (W×H×D, projections not included) | |
| **Weight** | | 1.1 kg (approximate; including BP-272) | |

\* Some frequency bands are not guaranteed.

**Transmitter**

|  |  |  |  |
| --- | --- | --- | --- |
| **Output power** |  | **13.8 V DC** | **7.4 V DC** |
| **SSB/CW/RTTY/FM/DV** | 0.1 to 10 W | 0.1 to 5 W |
| **AM** | 0.025 to 2.5 W | 0.025 to 1.25 W |
| **Modulation system** | | SSB : Digital PSN modulation  AM : Digital low power modulation  FM : Digital reactance modulation  DV : Digital GMSK modulation | |
| **Spurious emissions** | | Less than −50 dB (HF)  Less than −60 dB (50 MHz)  Less than −60 dB (144/430 MHz) | |
| **Carrier suppression** | | More than 50 dB | |
| **Unwanted sideband** | | More than 50 dB | |

**Receiver**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Receiver system** | **0.030 to 24.999 MHz** | RF Direct Sampling | | | |
| **25.000 MHz and above** | Down Conversion IF Sampling | | | |
| **Intermediate frequencies** | | 25.000 and above：38.85 MHz±0.5 MHz | | | |
| **Sensitivity (HF: Preamp-1 ON, 50 MHz: Preamp-2 ON, 144/430 MHz: Preamp ON)** |  | **0.500 to 1.799 MHz** | **1.800 to 29.999 MHz** | **50 MHz** | **144/430 MHz** |
| **SSB/CW（10 dB S/N)** | － | 0.20 μV | 0.15 μV | 0.11 μV |
| **AM（10dB S/N）13.0 μV** | 13.0 μV | 2.0 μV | 1.0 μV | 1.0 μV |
| **FM（12 dB SINAD）** | 0.5 μV (28.000 to 29.700 MHz) | | 0.25 μV | 0.18 μV |
| **DV（1% BER）（PN9）** | 1.0 μV (28.000 to 29.700 MHz) | | 0.63 μV | 0.35 μV |
| **Sensitivity for RED version (HF: Preamp-1 ON, 50 MHz: Preamp-2 ON, 144/430 MHz: Preamp ON)** |  | **1.8–2.999 MHz** | **3.0–29.995 MHz** | **50 MHz** | **144/430 MHz** |
| **SSB (BW=2.4 kHz)** | 10 dBμV emf | 0 dBμV emf | –6 dBμV emf | –6 dBμV emf |
| **AM (4 kHz, 60% modulation)** | 16 dBμV emf | 6 dBμV emf | 0 dBμV emf | 0 dBμV emf |
| **FM (7 kHz, 60% modulation)** | 0 dBμV emf (28.000 to 29.700 MHz) | | –6 dBμV emf | –6 dBμV emf |
| **Selectivity (Filter: SHARP)** | **SSB（BW=2.4 kHz）** | More than 2.4 kHz/－6 dB  Less than 3.4 kHz/－40 dB | | | |
| **CW（BW=500 Hz）** | More than 500 Hz/－6 dB  Less than 700 Hz/－40 dB | | | |
| **RTTY（BW=500 Hz）** | More than 500 Hz/－6 dB  Less than 800 Hz/－40 dB | | | |
| **AM（BW=6 kHz）** | More than 6.0 kHz/－6 dB  Less than 10 kHz/－40 dB | | | |
| **FM（BW=15 kHz）** | More than 12.0 kHz/－6 dB  Less than 22 kHz/－40 dB | | | |
| **DV（12.5 kHz spacing）** | Less than －50 dB | | | |
| **Spurious and image rejection ratio**  **(SSB/CW/AM/FM)** | | HF: More than 70 dB\* (except for ADC aliasing) 50 MHz: More than 70 dB\* 144 MHz: More than 65 dB 430 MHz: More than 54 dB \* At Intermediate frequency in 25–30 MHz or 50–54 MHz: More than 50 dB | | | |
| **Audio output power** | **Internal SP** | More than 530 mW (12 Ω load at 10% distortion) | | | |
| **External SP** | More than 200 mW (8 Ω load at 10% distortion) | | | |